LCcal

Costruction and Test of a new E.M. Calorimeter for a futur Linear Collider

Proposal

- Padova - LNF - help from DESY Requirements for ECAL in TDR di TESLA (LINEAR COLLIDER):

• high granularity,(Energy Flow) • σ_E O(10%/ √ E + 1%) • longitudinal segment. ( e/π) separation, • working in magnetic field • high density (25-30 X_0 in ∼ 50 cm) Solutions in TDR:

• Shashlik (thanx to CALEIDO) • Si W (Cost ??? 35 Mchann.???)

P. Checchia DESY 2000 09 24 1