LCcal

New Solution

New prototype

Keep Si W advantages:

• flat geometry (pointing software) • optimal shower-shower separation

Prototype Pb/Sc + Si:

• 50 layers:

• 25 × 25 × 0.3 cm^3 Pb • 25 × 25 × 0.3 cm^3 Scint.: 25 Cells 5 × 5 cm^2 • 3 planes:

• 625 1 × 1 cm^2 Si Pads • at: 2, 6, 12 X_0

P. Checchia DESY 2000 09 24 2